**Committee Name:** IPNNI Task Force

**Meeting Date:** November 5-7, 2019

**TITLE:** Propose Change to Section 5.3.4 of ATIS-1000074 v3

**SOURCE:** Perspecta Labs

**ISSUE NUMBER:**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**ABSTRACT:**

This contribution propose changes to the text in Section 5.3.4 of ATIS-1000074 v3 to improve clarity and minimize confusion. Specifically, it proposes to have separate paragraphs for aspects related to NS/EP NGN-PS and Emergency. Changes are shown as revision marks against IPNNI-2019-00130R001

# 1 Introduction

This contribution propose changes to the text in Section 5.3.4 of ATIS-1000074 v3 to improve clarity and minimize confusion. Specifically, it proposes to have separate paragraphs for aspects related to NS/EP NGN-PS and Emergency. Changes are shown as revision marks against IPNNI-2019-00130R001

# 2 Proposal

5.3.4 Handing of Calls with Signed SIP Resource Priority Header Field

For calls that contain a SIP Resource Priority Header (RPH) field, post STI-VS information may be passed for Call Validation Treatment (CVT) depending on the value of the namespace parameter in the RPH field and in accordance with local policy and/or policy of the authority responsible for the specific service.

**Emergency**

Calls with a SIP RPH value in the ‘esnet’ namespace may be passed for CVT depending on local policy.

**NS/EP NGN-PS**

Calls with a SIP RPH values in the ‘ets’ and ‘wps’ namespace shall not be passed for CVT. This is to ensure the highest probability of call completion for these types of calls.

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**