**ATIS-1000082.v002 (Draft)**

ATIS Standard on

**Technical Report on SHAKEN APIs for a Centralized Signing and Signature Validation Server**

**Alliance for Telecommunications Industry Solutions**

Approved TBD

**Abstract**

This document provides a Technical Report on a SHAKEN APIs used to support a Centralized Signing and Signature Validation Server. These APIs provide a means for multiple and/or disparate network elements to use an HTTP-based RESTful interface to access SHAKEN Signing and Signature Validation servers.

**Foreword**

The Alliance for Telecommunication Industry Solutions (ATIS) serves the public through improved understanding between providers, customers, and manufacturers. The Packet Technologies and Systems Committee (PTSC) develops and recommends standards and technical reports related to services, architectures, and signaling, in addition to related subjects under consideration in other North American and international standards bodies. PTSC coordinates and develops standards and technical reports relevant to telecommunications networks in the U.S., reviews and prepares contributions on such matters for submission to U.S. International Telecommunication Union Telecommunication Sector (ITU-T) and U.S. ITU Radiocommunication Sector (ITU-R) Study Groups or other standards organizations, and reviews for acceptability or per contra the positions of other countries in related standards development and takes or recommends appropriate actions.

The SIP Forum is an IP communications industry association that engages in numerous activities that promote and advance SIP-based technology, such as the development of industry recommendations, the SIPit, SIPconnect-IT, and RTCWeb-it interoperability testing events, special workshops, educational seminars, and general promotion of SIP in the industry. The SIP Forum is also the producer of the annual SIP Network Operators Conference (SIPNOC), focused on the technical requirements of the service provider community. One of the Forum's notable technical activities is the development of the SIPconnect Technical Recommendation – a standards-based SIP trunking recommendation for direct IP peering and interoperability between IP Private Branch Exchanges (PBXs) and SIP-based service provider networks. Other important Forum initiatives include work in Video Relay Service (VRS) interoperability, security, Network-to-Network Interoperability (NNI), and SIP and IPv6.

Suggestions for improvement of this document are welcome. They should be sent to the Alliance for Telecommunications Industry Solutions, PTSC, 1200 G Street NW, Suite 500, Washington, DC 20005, and/or to the SIP Forum, 733 Turnpike Street, Suite 192, North Andover, MA, 01845.

The mandatory requirements are designated by the word *shall* and recommendations by the word *should*. Where both a mandatory requirement and a recommendation are specified for the same criterion, the recommendation represents a goal currently identifiable as having distinct compatibility or performance advantages. The word *may* denotes an optional capability that could augment the standard. The standard is fully functional without the incorporation of this optional capability.

The **ATIS/SIP Forum IP-NNI Task Force** under the **ATIS** **Packet Technologies and Systems Committee (PTSC)** and the **SIP Forum** **Technical Working Group (TWG)** was responsible for the development of this document.

**Table of Contents**

1 Introduction 1

2 Normative References 1

3 Definitions, Acronyms, & Abbreviations 1

3.1 Definitions 2

3.2 Acronyms & Abbreviations 2

4 Architecture 2

5 General API Requirements 4

5.1 Resource Structure 4

5.2 Special Request Header Requirements 5

5.3 Special Response Header Requirements 5

6 Data Types 5

6.1 Datatype: signingRequest 5

6.2 Datatype: origTelephoneNumber 6

6.3 Datatype: destTelephoneNumber 6

6.4 Datatype: signingResponse 6

6.5 Datatype: verificationRequest 6

6.6 Datatype: serviceException 7

6.7 Datatype: verificationResponse 7

6.8 Datatype: exception 8

6.9 Datatype: policyException 8

6.10 Datatype: requestError 8

7 Exceptions 8

7.1 RESTful WebServices Exceptions 8

7.2 Service Exceptions 8

7.3 Policy Exceptions 9

8 API Interface 10

8.1 Signing API 10

8.1.1 Functional Behavior 10

8.1.2 Call Flow 11

8.1.3 Request (POST) 11

8.1.4 Response 12

8.2 Verification API 13

8.2.1 Functional Behavior 13

8.2.2 Call Flow 14

8.2.3 Request (POST) 15

8.2.4 Response 15

**Table of Figures**

Figure 4.1 – SHAKEN Reference Architecture 3

Figure 4.2 – SHAKEN STI-AS/STI-VS with Centralized Signing & Signature Validation Server 4

NOTE: Update TOC to include Appendix A

# Introduction

This technical report defines a Representational State Transfer (REST)ful interface that can be used in the Signature based Handling of Asserted information using toKENs (SHAKEN) framework to sign and verify telephony identity:

* Secure Telephone Identity Authentication Service (STI-AS) exposes an Applications Programming Interface (API) to sign the provided Personal Assertion Token (PASSporT) which includes the SHAKEN extension as defined in [draft-wendt-stir-passport-shaken].
* Secure Telephone Identity Verification Service (STI-VS) exposes an API to verify the signed Secure Telephone Identity (STI) according to procedures defined in IETF RFC 8225.

The only algorithm currently supported by this API is ES256.

The data set defined in this document could be expanded to accommodate other data types as needed (e.g., other PASSPort extensions that may need to be supported). Appendix A documents alternate data types and an API interface based on implementation experience gained since the original publication of this document.

Note that this is an informative document intended to provide illustrative examples of SHAKEN APIs. It is not intended to be normative and other implementation specific APIs may exist.

# Normative References

The following standards contain provisions which, through reference in this text, constitute provisions of this Standard. At the time of publication, the editions indicated were valid. All standards are subject to revision, and parties to agreements based on this Standard are encouraged to investigate the possibility of applying the most recent editions of the standards indicated below.

[Ref 1] IETF RFC 8225, *PASSporT: Personal Assertion Token.*[[1]](#footnote-1)

[Ref 2] PASSporT SHAKEN Extension.[[2]](#footnote-2)

[Ref 3] IETF RFC 8224, *Authenticated Identity Management in the Session Initiation Protocol (SIP).[[3]](#footnote-3)*

[Ref 4] ATIS-1000074, *Signature-based Handling of Asserted Information using toKENs (SHAKEN)*.[[4]](#footnote-4)

[Ref 5] ATIS-1000080, *Signature-based Handling of Asserted information using toKENs (SHAKEN): Governance Model and Certificate Management.[[5]](#footnote-5)*

# Definitions, Acronyms, & Abbreviations

For a list of common communications terms and definitions, please visit the *ATIS Telecom Glossary*, which is located at < <http://www.atis.org/glossary> >.

## Definitions

**Caller identity:** The originating phone number included in call signaling used to identify the caller for call screening purposes. In some cases, this may be the Calling Line Identification or Public User Identity.

## Acronyms & Abbreviations

|  |  |
| --- | --- |
| API | Applications Programming Interface |
| CSCF | Call Session Control Function |
| PASSporT | Personal Assertion Token |
| HTTP | HyperText Transfer Protocol |
| HTTPS | Hypertext Transfer Protocol Secure |
| IMS | IP Multimedia Subsystem |
| IP-NNI | ATIS and SIP Forum IP Network-to-Network Joint Task Force |
| ISC | IMS Service Control |
| ITU | International Telecommunication Union |
| ITU-T | U.S. International Telecommunication Union Telecommunication Sector |
| ITU-R | U.S. ITU Radiocommunication Sector |
| JSON | JavaScript Object Notation |
| NNI | Network-to-Network Interoperability |
| PBXs | IP Private Branch Exchanges |
| PTSC | The Packet Technologies and Systems Committee |
| REST | Representational State Transfer |
| SHAKEN | Signature based Handling of Asserted information using toKENs |
| SIP | Session Initiation Protocol |
| SIPNOC | SIP Network Operators Conference |
| SKS | Secure Key Store |
| STI | Secure Telephone Identity |
| STI-AS | Secure Telephone Identity Authentication Service |
| STI-CR | Secure Telephone Identity Certificate Repository |
| STI-VS | Secure Telephone Identity Verification Service |
| STIR | Secure Telephone Identity Revisited |
| TWG | Technical Working Group |
| UTC | Coordinated Universal Time |
| UUID | Universally Unique Identifier |
| VRS | Video Relay Service |

# Architecture

Figure 4.1 depicts the SHAKEN reference architecture as described in Reference [4]. The reference architecture is based on the 3GPP IP Multimedia Subsystem (IMS) architecture, whereby the STI-AS and STI-VS are shown as IMS Application Servers, connecting to the IMS core Call Session Control Function (CSCF) via Session Initiation Protocol (SIP) IMS Service Control (ISC) interfaces.



Figure 4.1 – SHAKEN Reference Architecture

As service providers incorporate SHAKEN into their infrastructure, they may need to deploy SHAKEN capabilities into multiple networks; some networks may be IMS-based, and some may not. Furthermore, service providers may determine that the STI-AS and/or STI-VS functions are better suited to be invoked at points other than the network core, such as at the network edge. The use of SIP as the STI-AS/STI-VS access protocol may not be suitable when initiating authentication and/or verification requests from locations other than an IMS core.

Because of the potential need for a service provider to initiate authentication and verification in multiple networks and/or from different network elements within their infrastructure, it would be beneficial to share a centralized authentication and verification service, calling upon these services from various points within a service provider’s infrastructure.

This technical report describes a means of decomposing the STI-AS and STI-VS functions and exposing a HyperText Transfer Protocol (HTTP)-based RESTful API that can be used to request SHAKEN authentication and verification services. The API can be used by diverse network elements within a service provider’s network to make SHAKEN authentication and verification requests of shared, centralized Signing and Signature Validation servers.

As shown in Figure 4.2, the overall STI-AS functionality is decomposed into two parts: a Signing server function and an authenticator function. Likewise, the STI-VS is decomposed into a Signature Validation server function and a verifier function. The HTTP-based API is used between the authenticator and Signing server functions and between the verifier and Signature Validation server functions. Figure 4.2 depicts a combined Signing and Signature Validation Server function, but this is optional.

The authenticator and verifier functions initiate the signing and validation requests via the API described in this document. The authenticator and verifier functions may be integrated into other network elements or may be developed as stand-alone functions. For example, a stand-alone authenticator function in an implementation of the SHAKEN reference architecture would receive SIP INVITE messages from the CSCF and formulate and send an HTTP signing request to the Signing server per the API described in this document. The Signing server performs the signing/authentication functions and formulates an API response containing an Identity header that the authenticator adds to the SIP INVITE message returned to the CSCF. Alternatively, the authenticator function could be integrated into the CSCF, whereby the CSCF would directly support the new API.



Figure 4.2 – SHAKEN STI-AS/STI-VS with Centralized Signing & Signature Validation Server

# General API Requirements

1. STI-AS and STI-VS have to expose RESTful web services implemented using HTTP and aligned with the principles of RESTful API.
2. Only JavaScript Object Notation (JSON)-based data format is supported. APIs use “application/json” content type.
3. All validations will be described below in the error handling sections for each API explicitly.
4. POST HTTP request is used for both APIs.
5. HTTP 1.1 protocol version has to be supported by server side.

## Resource Structure

REST resources are defined with respect to a “server Root”:

“serverRoot” = http://{hostname}:{port}/{optionalRoutingPath}

The resource structure is provided below:



‘apiVersion’ should be set to “1”.

## Special Request Header Requirements

The following headers are expected to be sent in all HTTP requests:

| Header Name | Mandatory? | Description |
| --- | --- | --- |
| X-RequestID | N | The **X-RequestID** transaction ID should be included in order to make possible the transaction traceability in case of troubleshooting and fault analysis.  If received, it will not be validated explicitly by server. If not received, it will be automatically generated by STI-AS/VS service on request receipt.  Received/Generated transaction ID will be returned back in the corresponding HTTP response in “X-RequestID” header. |
| X-InstanceID | N | For auditing purposes, each component calling the API should identify itself by sending its identity (e.g., VNFC name/UUID, VM name/UUID ...) in "**X-InstanceID**" header. |
| Content-Type | Y | Determines the format of the request body.  Valid value is: “**application/json**”.  Requests with other types will be rejected with “415 Unsupported Media type” HTTP status code. |
| Accept | N | If specified, has to contain “**application/json**” content type, otherwise HTTP request will be rejected with “406 Not Acceptable” HTTP Status Code.  If not specified, will be default handled as “**application/json**”. |

## Special Response Header Requirements

The following headers are expected to be sent in all HTTP responses:

| Header Name | Mandatory? | Description |
| --- | --- | --- |
| X-RequestID | Y | Received/Generated **X-RequestID** transaction ID will be returned back in the corresponding HTTP response. |
| Content-Type | Y | Determines the format of the response body.  Valid value is: **“application/json”**. |

# Data Types

## Datatype: signingRequest

| Key Name | Key Value Type | Required? | Description |
| --- | --- | --- | --- |
| attest | String  Allowed values:  [“A”, “B”, “C”] | Y | SHAKEN extension to PASSporT.  Indicator identifying the service provider that is vouching for the call as well as clearly indicating what information the service provider is attesting to.  SHAKEN spec requires “attest” key value be set to uppercase characters “A”, “B”, or “C”. |
| dest | destTelephoneNumber | Y | Represents the called party. Array containing **one or more** identities of TNs. |
| iat | Integer | Y | “Issued At Claim”: Should be set to the date and time of issuance of the PASSporT Token.  The time value should be in the Numeric Date format defined in RFC 7519: number of seconds elapsed since 00:00:00 Coordinated Universal Time (UTC), Thursday, 1 January 1970 not including leap seconds. |
| orig | origTelephoneNumber | Y | Represents the asserted identity of the originator of the personal communications signaling. |
| origid | String | Y | The unique origination identifier (“origid”) is defined as part of SHAKEN extension to PASSporT. This unique origination identifier should be a globally unique string corresponding to a UUID (RFC 4122). |

## Datatype: origTelephoneNumber

| Field | Type | Required? | Description |
| --- | --- | --- | --- |
| tn | String  Allowed Characters :  [0-9],\*,#,+, and  visual separators defined in  RFC 3966: “.”, “-“, “(“, “)”. | Y | Telephone Number of Originating identity.  Server will remove all non-numeric characters if received except star (\*) and pound (#) characters.  Ex.: (+1) 235-555-1212 🡪 12355551212 |

## Datatype: destTelephoneNumber

|  |  |  |  |
| --- | --- | --- | --- |
| Field | Type | Required? | Description |
| tn | List of Strings  [1 … unbounded]  Allowed Characters:  [0-9],\*,#,+, and  visual separators defined in  RFC 3966: “.”, “-“, “(“, “)”. | Y | Telephone Number(s) of Destination identity.  List containing **one or more** identities of String type.  Server will remove all non-numeric characters if received except star (\*) and pound (#) characters.  Ex.: (+1) 235-555-1212 🡪 12355551212 |

## Datatype: signingResponse

|  |  |  |  |
| --- | --- | --- | --- |
| Key Name | Key Value Type | Required? | Description |
| identity | String  Cannot be NULL | Y | Identity header value as defined in RFC 8224 with “identityDigest” in full format and mandatory “info” parameter. The “info” header field parameter contains the public key URL of the certificate used during STI signing. |

## Datatype: verificationRequest

| Key Name | Key Value Type | Required? | Description |
| --- | --- | --- | --- |
| identity | String | Y | Identity header value as defined in RFC 8224 with “identityDigest” in full format and mandatory “info” parameter. |
| to | destTelephoneNumber | Y | Represents the called party. Array containing **one or more** identities of destination TNs. This is set to the value of the “To:” header field parameter in the incoming SIP Invite. |
| time | Integer | Y | This is set based on the value of the Date header field parameter in the incoming Invite.  The time value should be in the Numeric Date format defined in RFC 7519: number of seconds elapsed since 00:00:00 UTC, Thursday, 1 January 1970 not including leap seconds. |
| from | origTelephoneNumber | Y | Represents the asserted identity of the originator of the personal communications signaling.  This is set to the value of the “P-Asserted-Identity”, if available, or “From” header field parameter in the incoming Invite. |

## Datatype: serviceException

|  |  |  |  |
| --- | --- | --- | --- |
| Field | Type | Required? | Description |
| serviceException | exception | Y | Service Exception. |

## Datatype: verificationResponse

| Key Name | Key Value Type | Required? | Description |
| --- | --- | --- | --- |
| reasoncode | Integer | N | Reason Code to be used in case of failed verification by STI-VS to build SIP Reason header if required.  Currently possible values are defined as follows:  403,  428 (recommendation is to not use this Reason Code until a point where all calls on the VoIP network are mandated to be signed),  436,  437,  438. |
| reasontext | String | N | Reason Text to be used in case of failed verification by STI-VS to build SIP Reason header if required.  Currently possible values are defined as follows:  403 - “Stale Date”  428 - “Use Identity Header” (recommendation is to not use this Reason Text until a point where all calls on the VoIP network are mandated to be signed)  436 – “Bad Identity Info”  437 – “Unsupported Credential”  438 – “Invalid Identity Header” |
| reasondesc | String | N | Reason details description. Can be used for logging and troubleshooting. |
| verstat | String  {“TN-Validation-Passed”,  “TN-Validation-Failed”,  “No-TN-Validation”} | Y | Verification Status:  **TN-Validation-Passed** - The number passed the validation.  **TN-Validation-Faile**d - The number failed the validation.  **No-TN-Validation** - No number validation was performed. |

## Datatype: exception

| Field | Type | Required? | Description |
| --- | --- | --- | --- |
| messageId | string | Yes | Unique message identifier of the format ‘ABCnnnn’ where ‘ABC’ is either ‘SVC’ for Service Exceptions or ‘POL’ for Policy Exception. Exception numbers may be in the range of 0001 to 9999 where 0001 to 2999 are defined by the Open Mobile Alliance and 3000-9999 are available and undefined. |
| text | string | Yes | Message text, with replacement variables marked with %n, where n is an index into the list of <variables> elements, starting at 1. |
| variables | string | No | List of zero or more strings that represent the contents of the variables used by the message text. |
| url | string | No | Hyperlink to a detailed error resource e.g., an HTML page for browser user agents. Currently will not be used. |

## Datatype: policyException

|  |  |  |  |
| --- | --- | --- | --- |
| Field | Type | Required? | Description |
| policyException | exception | Yes | Policy Exception. |

## Datatype: requestError

|  |  |  |  |
| --- | --- | --- | --- |
| Field | Type | Required? | Description |
| requestError | policyException or serviceException | Yes | Request Error Message. |

# Exceptions

## RESTful WebServices Exceptions

RESTful services generate and send exceptions to clients in response to invocation errors. Exceptions send HTTP status codes (specified later in this document for each operation). HTTP status codes may be followed by an optional JSON exception structure (“requestError” datatype). Two types of exceptions may be defined: service exceptions and policy exceptions.

## Service Exceptions

When a service is not able to process a request, retrying the request with the same information will also result in a failure, and the issue is not related to a service policy issue, then the service will issue a fault using the service exception fault message. Examples of service exceptions include invalid input, lack of availability of a required resource, or a processing error.

A service exception uses the letters 'SVC' at the beginning of the message identifier. ‘SVC’ service exceptions used by SHAKEN API are defined below:

| Exception  ID | Exception text | HTTP Status Code | Exception  Variables | Error Description |
| --- | --- | --- | --- | --- |
| SVC4000 | Error: Missing request body. | 400 | - | **MISSING\_BODY**  The API failed due to missing body. |
| SVC4001 | Error: Missing mandatory parameter ‘%1’. | 400 | %1 – parameter name | **MISSING\_INFORMATION**  The API failed due to missing mandatory parameter. |
| SVC4002 | Error: Requested response body type ‘%1’ is not supported. | 406 | %1 – not supported response body type | **NOT\_ACCEPTABLE\_RESPONSE\_BODY\_TYPE**  A request was made of a resource for a non-supported message body format. |
| SVC4003 | Error: Requested resource was not found. | 404 | - | **RESOURCE\_NOT\_FOUND**  The server has not found anything matching the Request-URI. |
| SVC4004 | Error: Unsupported request body type, expected ‘%1’. | 415 | %1 – content type  (’application/json’) | **UNSUPPORTED\_REQUEST\_BODY\_TYPE**  Received unsupported message body type. |
| SVC4005 | Error: Invalid ‘%1’ parameter value: %2. | 400 | %1 – parameter name  %2– short error description | **INVALID\_PARAMETER\_VALUE**  Parameter’s value is invalid. |
| SVC4006 | Error: Failed to parse received message body: %1. | 400 | %1-“invalid message body length specified”/”invalid JSON body” | **FAILED\_TO\_PARSE\_MSG\_BODY** |
| SVC4007 | Error: Missing mandatory Content-Length header | 411 | - | **MISSING\_BODY\_LENGTH**  The Content-Length header was not specified. |

## Policy Exceptions

When a service is not able to complete because the request fails to meet a policy criteria, then the service will issue a fault using the policy exception fault message. To clarify how a policy exception differs from a service exception, consider that all the input to an operation may be valid as meeting the required input for the operation (thus no service exception), but using that input in the execution of the service may result in conditions that require the service not to complete. Examples of policy exceptions include API violations, requests not permitted under a governing service agreement, or input content not acceptable to the service provider.

A Policy Exception uses the letters 'POL' at the beginning of the message identifier. ‘POL’ policy exceptions used by SHAKEN API are defined below:

| Exception  ID | Exception text | HTTP Status Code | Exception  Variables | Error Description |
| --- | --- | --- | --- | --- |
| POL4050 | Error: Method not allowed | 405 | - | The resource was invoked with unsupported operation. |
| POL5000 | Error: Internal Server Error. Please try again later. | 500 | - | The request failed due to internal error. |

# API Interface

## Signing API

### Functional Behavior

Used to create the PASSporT signature with private key certificate.

The Authenticator sends a signingRequest including the following to the SHAKEN Signing Service:


1. The “orig” parameter is populated using the PAI field if present, otherwise using the From header field in the SIP Invite.
2. The “dest” parameter is populated using the To header field in the SIP Invite.
3. The “iat” parameter is populated using the “Date” header field in the SIP Invite. If there is no “Date” header field in the SIP Invite, a Date header field is added to the SIP INVITE.
4. The “origid” parameter is determined as described in ATIS-1000074 for the “origid” field in the PASSporT.
5. The “attest” parameter is determined as described in ATIS-1000074 for the “attest” field in the PASSporT.
6. The signingRequest is then sent to the SHAKEN Signing Service.

The SHAKEN Signing Service performs the following steps:

1. Validate the incoming signing request parameters in terms of parameter’s type and format.
2. Validate the “iat” parameter value in terms of “freshness”: the request with “iat” value with time different by more than one minute from the current time will be rejected.
3. Normalize to the canonical form the received telephony numbers if needed (remove visual separators and leading “+”).
4. Build SHAKEN PASSport protected JWT header (with “ppt” SHAKEN extension).
5. Build SHAKEN PASSporT JWT payload by keeping lexicographic order and removing space and line breaking characters.
6. Generate PASSporT signature with appropriate certificate private key.
7. Build Full Form of PASSporT.
8. Build SIP “Identity” header value by using identity digest from the previous step and add “info” parameter with angle bracketed URI used to acquire the public key of certificate used during PASSporT signing.
9. If successfully signed, build and send “signingResponse” to the Authenticator, otherwise send error.

Upon receipt of the signingResponse, the Authenticator uses the “identity” parameter in the response to populate the SIP Identity header field and forwards the request. If no identity parameter is received in a response, the Authenticator forwards the request without adding a SIP Identity header field.

### Call Flow



### Request (POST)

The used resource is: http://{serverRoot}/stir/v1/signing.

|  |  |
| --- | --- |
| Name | Description |
| serverRoot | Server base URL: hostname+port+base path  Hostname contains the Global FQDN of Signing Service. |

#### Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Signing Request | signingRequest | Yes | Contains the JSON structure of the signing request (PASSporT payload claims). |

#### Request Sample

POST /stir/v1/signing HTTP/1.1

Host: stir.example.com

Accept: application/json

X-InstanceID : de305d54-75b4-431b-adb2-eb6b9e546014

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"signingRequest”: {

"attest": “A”,

"orig”: {

“tn”: “12155551212”

},

“dest”: {

“tn”: [

“12355551212”

]

},

"iat”: 1443208345,

“origid”: “de305d54-75b4-431b-adb2-eb6b9e546014”

}

}

### Response

#### Response Body

Response body is returned as JSON object (Content-Type: application/json).

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Signing Response | signingResponse | Yes | Contains the JSON structure of the signing response (SIP Identity header field value). |

#### Response Sample (Success)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"signingResponse": {

"identity": “eyJhbGciOiJFUzI1NiIsInR5cCI6InBhc3Nwb3J0IiwicHB0Ijoic2hha2VuIiwieDV1IjoiaHR0cDov L2NlcnQtYXV0aC5wb2Muc3lzLmNvbWNhc3QubmV0L2V4YW1wbGUuY2VydCJ9eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6IisxMjE1NTU1MTIxMyJ9LCJpYXQiOiIxNDcxMzc1NDE4Iiwib3JpZyI6eyJ0biI64oCdKzEyMTU1NTUxMjEyIn0sIm9yaWdpZCI6IjEyM2U0NTY3LWU4OWItMTJkMy1hNDU2LTQyNjY1NTQ0MDAwMCJ9.\_28kAwRWnheXyA6nY4MvmK5JKHZH9hSYkWI4g75mnq9Tj2lW4WPm0PlvudoGaj7wM5XujZUTb\_3MA4modoDtCA;info=<<https://cert.example2.net/example.cert>>”

}

}

#### Response Sample (Failure)

HTTP/1.1 400 Bad Request

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

“requestError”: {

“serviceException”: {

“messageId”: “SVC4001”

“text”: “Error: Missing mandatory parameter ‘%1’”,

“variables”: [“iat”]

}

}

}

#### HTTP Response Codes

|  |  |  |
| --- | --- | --- |
| Response code | Service/Policy  Exception | Reason /Description |
| 200 | N/A | Successful signing. |
| 400 | SVC4000 | Missing JSON body in the request. |
| 400 | SVC4001 | Missing mandatory parameter. |
| 406 | SVC4002 | Not supported body type is specified in Accept HTTP header. |
| 415 | SVC4004 | Received unsupported message body type in Content-Type HTTP header. |
| 400 | SVC4005 | Invalid parameter value. |
| 400 | SVC4006 | Failed to parse JSON body. |
| 411 | SVC4007 | Missing mandatory Content-Length header. |
| 405 | POL4050 | Method Not Allowed: Invalid HTTP method used (all methods except POST will be rejected for the specific resource URL). |
| 500 | POL5000 | The POST request failed due to internal signing server problem. |

## Verification API

### Functional Behavior

The Verification API is used to verify the signature provided in the Identity header field and to determine that the signing service credentials demonstrate authority over the call originating identity.


Upon receipt of a SIP INVITE containing a SIP Identity header field parameter, the Verifier builds a verificationRequest as follows:

1. The “from” parameter is populated using the PAI field if present, otherwise using the From header field in the SIP Invite.
2. The “to” parameter is populated with the To header field from the SIP Invite.
3. The “time” parameter value is populated with the RFC7519 encoded Date header field from the SIP Invite.
4. The “identity” parameter value is populated using the Identity header field in the SIP Invite.
5. The Verifier then sends the HTTP Post to request verification.

Upon receipt of the verificationRequest, the SHAKEN Verification Service performs the following steps. Each step is associated with the appropriate error case(s) specified in the section “Mapping of verification failure cases to the returned SIP header parameters”. The error case numbers **En** per each step is specified in parentheses.

1. Validate the incoming verification request parameters in terms of parameter’s type and format (E1 and E2).
2. Validate the “time” parameter value in terms of “freshness”: a request with a “time” value which is different by more than one minute from the current time will be rejected (E3).
3. Parse the “identity” parameter value:
   1. full form of PASSporT is required by SHAKEN: “identity-digest” parameter of Identity header has to be parsed to validate the full form format [three data portions delimited with dot (“.”)]. If the expected format is not matched 🡪 reject request on the Invalid PASSporT form (E4).
   2. If “ppt” parameter is specified and its value is not “shaken” 🡪 reject request (E5).
   3. If “info” parameter is not specified 🡪 reject request (E6).
   4. If the URI specified in “info” parameter is not syntactically valid 🡪 reject request (E7).
4. Decode “identity-digest” parameter value to extract from the first portion (PASSporT header) “ppt”, “typ”, ”alg” and “x5u” claims:
   1. If one of the mentioned claims is missing -> reject request (E9).
   2. If extracted “typ” value is not equal to “passport” 🡪 reject request (E11).
   3. If extracted “alg” value is not equal to “ES256” 🡪 reject request (E12).
   4. If extracted “x5u” value is not equal to the URI specified in the “info” parameter of Identity header 🡪 reject request (E10).
   5. If extracted “ppt” is not equal to “shaken” 🡪 reject request (E13).
5. Decode “identity-digest” parameter value to extract from the second portion (PASSporT payload) “dest”, “orig”, “attest”, “origid” and “iat” claims:
   1. On missing mandatory claims reject request (E14).
   2. Validate the extracted from payload “iat” claim value in terms of “freshness” relative to “time” value: request with “expired” “iat” will be rejected🡪 reject request (E15).
   3. On invalid “attest” claim reject request (E19).
   4. Normalize to the canonical form the received in the “verificationRequest” “from” and “to” telephone numbers (remove visual separators and leading “+”) and compare them with ones extracted from the “orig” and “dest” claims of PASSporT payload. If they are not identical 🡪 reject request (E16).
6. Dereference “info” parameter URI to a resource that contains the public key of the certificate used by signing service to sign a request. If there is a failure to dereference the URI due to timeout or a non-existent resource, the request is rejected (E8).
7. Validate the issuing CA. On the failure to authenticate the CA (for example not valid, no root CA) request will be rejected (E17).
8. Validate the signature of “identity” digest parameter. On failure, reject the request (E18).

### Call Flow



### Request (POST)

The used resource is: http://{serverRoot}/stir/v1/verification.

|  |  |
| --- | --- |
| Name | Description |
| serverRoot | Server base URL: hostname+port+base path.  Hostname contains the Global FQDN of Verification Service. |

#### Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Verification Request | verificationRequest | Yes | Contains the JSON structure of the verification request (PASSporT payload claims + identity header). |

#### Request Sample

POST /stir/v1/verification HTTP/1.1

Host: stir.example.com

Accept: application/json

X-InstanceID : de305d54-75b4-431b-adb2-eb6b9e546014

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

“verificationRequest”: {

“from”: {

“tn”: “12155551212”

},

“to”: {

“tn”: [

“12355551212”

]

},

“time”: 1443208345,

“identity”: “eyJhbGciOiJFUzI1NiIsInR5cCI6InBhc3Nwb3J0IiwicHB0Ijoic2hha2VuIiwieDV1IjoiaHR0cDov L2NlcnQtYXV0aC5wb2Muc3lzLmNvbWNhc3QubmV0L2V4YW1wbGUuY2VydCJ9eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6IisxMjE1NTU1MTIxMyJ9LCJpYXQiOiIxNDcxMzc1NDE4Iiwib3JpZyI6eyJ0biI64oCdKzEyMTU1NTUxMjEyIn0sIm9yaWdpZCI6IjEyM2U0NTY3LWU4OWItMTJkMy1hNDU2LTQyNjY1NTQ0MDAwMCJ9.\_28kAwRWnheXyA6nY4MvmK5JKHZH9hSYkWI4g75mnq9Tj2lW4WPm0PlvudoGaj7wM5XujZUTb\_3MA4modoDtCA;info=<<https://cert.example2.net/example.cert>>”

}

}

### Response

#### Response Body

Response body is returned as JSON object (Content-Type: application/son).

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Verification Response | verificationResponse | Yes | Contains the JSON structure of the verification response. |

#### Mapping of Verification Failure Cases to the Returned SIP Reason Header Field Parameters

| Error Case Number | Error Case  (“reasondesc”) | HTTP Status Code | “reasoncode” | “reasontext” | “verstat” |
| --- | --- | --- | --- | --- | --- |
| E1 | Missing mandatory parameters in the verification request  (“from”, “to”, “time”, “identity”). | 400 with service exception | - | - | No-TN-Validation |
| E2 | Received invalid parameters  (invalid “from”/“to” tn format, “time” value). | 400 with service exception | - | - | No-TN-Validation |
| E3 | Received ‘iat’ value is not fresh. | 200 | 403 | Stale Date | No-TN-Validation |
| E4 | Identity header in compact form instead of required by SHAKEN spec full form. | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E5 | Identity header is received with ‘ppt’ parameter value that is not ‘shaken’. | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E6 | Missing ‘info’ parameter in the ‘identity’. | 200 | 436 | Bad identity Info | No-TN-Validation |
| E7 | Invalid ‘info’ URI. | 200 | 436 | Bad identity Info | No-TN-Validation |
| E8 | Failed to dereference ‘info’ URI. | 200 | 436 | Bad identity Info | No-TN-Validation |
| E9 | Missing ‘%1’ claim in the PASSporT header.  %1 - “ppt”, ”typ”, ”alg”, ”x5u” | 200 | 436 | Bad identity Info | No-TN-Validation |
| E10 | ‘x5u’ from PASSporT header doesn’t match the ‘info’ parameter of identity header value. | 200 | 436 | Bad identity Info | No-TN-Validation |
| E11 | ‘typ’ from PASSporT header is not ‘passport’. | 200 | 437 | Unsupported credential | No-TN-Validation |
| E12 | ‘alg‘ from PASSporT header is not ‘ES256’. | 200 | 437 | Unsupported credential | No-TN-Validation |
| E13 | ‘ppt‘ from PASSporT header is not ‘shaken’. | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E14 | Missing ‘%1’ mandatory claim in PASSporT payload  %1 - “dest”, “orig”, “attest”, “origid”, “iat” | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E15 | ‘iat’ from PASSporT payload is not fresh. | 200 | 403 | Stale Date | No-TN-Validation |
| E16 | ‘%1’ claim from PASSporT payload doesn’t match the received in the verification request claim.  %1 - “orig”, “dest” | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E17 | Failed to authenticate CA. | 200 | 437 | Unsupported credential | TN-Validation-Failed |
| E18 | Signature validation failed. | 200 | 438 | Invalid Identity Header | TN-Validation-Failed |
| E19 | ‘attest’ claim in PASSporT payload is not valid. | 200 | 438 | Invalid Identity Header | No-TN-Validation |

#### Response Sample (Success + Successful Validation)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"verificationResponse": {

“verstat”: “TN-Validation-Passed”

}

}

#### Response Sample (Success + Failed Validation)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"verificationResponse": {

“reasoncode”: 436,

“reasontext”: “Bad Identity Info”,

“reasondesc”: “Invalid ‘info’ URI”,

“verstat”: “No-TN-Validation”

}

}

#### Response Sample (Failure)

HTTP/1.1 400 Bad Request

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

“requestError”: {

“serviceException”: {

“messageId”: “SVC4001”

“text”: “Error: Missing mandatory parameter ‘%1’”,

“variables”: [“iat”]

}

}

}

#### HTTP Response Codes

| Response code | Service/Policy  Exception | Reason /Description |
| --- | --- | --- |
| 200 | N/A | Successful signing. |
| 400 | SVC4000 | Missing JSON body in the request. |
| 400 | SVC4001 | Missing mandatory parameter. |
| 406 | SVC4002 | Not supported body type is specified in Accept HTTP header. |
| 415 | SVC4004 | Received unsupported message body type in Content-Type HTTP header. |
| 400 | SVC4005 | Invalid parameter value. |
| 400 | SVC4006 | Failed to parse JSON body. |
| 411 | SVC4007 | Missing mandatory Content-Length header. |
| 405 | POL4050 | Method Not Allowed: Invalid HTTP method used (all methods except POST will be rejected for the specific resource URL). |
| 500 | POL5000 | The POST request failed due to internal signing server problem. |

# Appendix A – Alternate API

The following alternate API is based on implementation experience since the original publication of this document in May 2018.

This API is based on the architecture described in section 4, however offers variations to the following:

* Section 5: General API Requirements
  + The Resource Structure allows support for the bundling of signing and verification requests
* Section 6: Data Types
  + Supports ppt extensions (including div) and URI format
* Section 7: Exceptions
  + Handled within the context of the Data Types
* Section 8: API interface
  + Due to changes in data types and exception handling.

# General API Requirements


1. STI-AS and STI-VS have to expose RESTful web services implemented using HTTP and aligned with the principles of RESTful API.
2. Only JSON based data format is supported. APIs use “application/json” content type
3. All validations will be described below in the error handling sections for each API explicitly.
4. POST HTTP request is used for both APIs.
5. HTTP 1.1 protocol version has to be supported by server side.

## Resource Structure

REST resources are defined with respect to a “server Root”:

“serverRoot” = http://{hostname}:{port}/{optionalRoutingPath}

The resource structure is provided below:



‘apiVersion’ should be set to “1”.

## Special Request Header Requirements

The following headers are expected to be sent in all HTTP requests:

| Header Name | Mandatory? | Description |
| --- | --- | --- |
| X-RequestID | N | The **X-RequestID** transaction ID should be included in order to make possible the transaction traceability in case of troubleshooting and fault analysis.  If received, it will not be validated explicitly by server. Received transaction ID will be returned back in the corresponding HTTP response in “X-RequestID” header. |
| X-InstanceID | N | For auditing purposes, each component calling the API should identify itself by sending its identity (e.g., VNFC name/UUID, VM name/UUID ...) in "**X-InstanceID**" header. |
| Content-Type | Y | Determines the format of the request body.  Valid value is: “**application/json**”.  Requests with other types will be rejected with “415 Unsupported Media type” HTTP status code. |
| Accept | N | If specified, has to contain “**application/json**” content type, otherwise HTTP request will be rejected with “406 Not Acceptable” HTTP Status Code.  If not specified, will be default handled as “**application/json**”. |

## Special Response Header Requirements

The following headers are expected to be sent in all HTTP responses:

| Header Name | Mandatory? | Description |
| --- | --- | --- |
| X-RequestID | N | Received **X-RequestID** transaction ID will be returned back in the corresponding HTTP response. |
| Content-Type | Y | Determines the format of the response body.  Valid value is: **“application/json”** |

# Data Types

## Datatype: signingRequest

|  |  |  |  |
| --- | --- | --- | --- |
| Key Name | Key Value Type | Required? | Description |
| attest | String | N | SHAKEN extension to PASSporT.  Indicator identifying the service provider that is vouching for the call as well as clearly indicating what information the service provider is attesting to.  SHAKEN spec requires “attest” key value be set to uppercase characters “A”, “B”, or “C”.  This must be present if, and only if, **ppt** is "shaken" or omitted. |
| dest | destAddress | Y | Represents the called party. Array containing **one or more** identities of TNs. |
| div | divAddress | N | Represents the party this call has been diverted from.  This must be present if, and only if, **ppt** is "div". |
| iat | Integer | Y | “Issued At Claim”: Should be set to the date and time of issuance of the PASSporT Token.  The time value should be in the Numeric Date format defined in RFC 7519: number of seconds elapsed since 00:00:00 Coordinated Universal Time (UTC), Thursday, 1 January 1970 not including leap seconds. |
| orig | origAddress | Y | Represents the asserted identity of the originator of the personal communications signaling. |
| origid | String | N | The unique origination identifier (“origid”) is defined as part of SHAKEN extension to PASSporT. This unique origination identifier should be a globally unique string corresponding to a UUID (RFC 4122).  This must be present if, and only if, **ppt** is "shaken" or omitted. |
| ppt | String  Allowed values:  ["shaken", "div"] | N | Represents the extension to use when creating this PASSporT, this places restrictions on the other fields passed into this request. |
| profileid | String | N | Identifier of the profile in the profile table on the server to use for signing this request.  This profile determines configuration used for signing, e.g. signing key, public certificate URL, required IAT freshness. |
| requestid | String | N | An opaque identifier that is reflected in the response in order to make possible the transaction traceability in case of troubleshooting and fault analysis. |

## Datatype: origAddress

| Field | Type | Required? | Description |
| --- | --- | --- | --- |
| tn | String  Allowed Characters :  [0-9],\*,#,+, and  visual separators defined in  RFC 3966 : “.”, “-“, “(“, “)”. | N | Telephone Number of Originating identity.  Server will remove all non-numeric characters if received except star (\*) and pound (#) characters.  Ex. : (+1)235-555-1212 🡪 12355551212 |
| uri | String  As defined in RFC 3261 Section 19.1 | N | SIP or SIPS URI address of originating party.  Must be of the form ( "sip" / "sips" ) ":" user "@" host, all in lower case, and any percent-encoded octets decoded. |

## Datatype: divAddress

| Field | Type | Required? | Description |
| --- | --- | --- | --- |
| tn | String  Allowed Characters :  [0-9],\*,#,+, and  visual separators defined in  RFC 3966 : “.”, “-“, “(“, “)”. | N | Telephone Number of diverting identity.  Server will remove all non-numeric characters if received except star (\*) and pound (#) characters.  Ex. : (+1)235-555-1212 🡪 12355551212 |
| uri | String  As defined in RFC 3261 Section 19.1 | N | SIP or SIPS URI address of diverting party.  Must be of the form ( "sip" / "sips" ) ":" user "@" host, all in lower case, and any percent-encoded octets decoded. |

## Datatype: destAddress

|  |  |  |  |
| --- | --- | --- | --- |
| Field | Type | Required? | Description |
| tn | List of Strings  [1 … unbounded]  Allowed Characters:  [0-9],\*,#,+, and  visual separators defined in  RFC 3966: “.”, “-“, “(“, “)”. | N | Telephone Number(s) of Destination identity  List containing **one or more** identities of String type.  Server will remove all non-numeric characters if received except star (\*) and pound (#) characters.  Ex.: (+1)235-555-1212 🡪 12355551212 |
| uri | List of Strings  [1 … unbounded]  As defined in RFC 3261 Section 19.1 | N | SIP or SIPS URI(s) address of destination party.  List containing **one or more** identities of String type.  Each element must be of the form ( "sip" / "sips" ) ":" user "@" host, all in lower case, and any percent-encoded octets decoded. |

## Datatype: signingResponse

|  |  |  |  |
| --- | --- | --- | --- |
| Key Name | Key Value Type | Required? | Description |
| identity | String  Cannot be NULL | Y | Identity header value as defined in RFC 8224 with “identityDigest” in full format and mandatory “info” parameter. The “info” header field parameter contains the public key URL of the certificate used during STI signing. |
| errorid | String | N | Alphanumeric identifier indicating the nature of the error. |
| reasoncode | Integer | N | Reason Code to be used in case of failed signing. Can be used for logging and troubleshooting. |
| reasontext | String | N | Reason Text to be used in case of failure. Can be used for logging and troubleshooting. |
| reasondesc | String | N | Reason details description. Can be used for logging and troubleshooting. |
| requestid | String | N | An opaque identifier that is reflected from the request in order to make possible the transaction traceability in case of troubleshooting and fault analysis. |

## Datatype: verificationRequest

| Key Name | Key Value Type | Required? | Description |
| --- | --- | --- | --- |
| identity | String | N | Identity header value as defined in RFC 8224 with “identityDigest” in full format and mandatory “info” parameter. |
| identities | List of Strings | N | List of all identity header values as defined in RFC 8224 with “identityDigest” in full format and mandatory “info” parameter. |
| to | destAddress | Y | Represents the called party. Array containing **one or more** identities of destination TNs. This is set to the value of the “To:” header field parameter in the incoming SIP Invite. |
| time | Integer | Y | This is set based on the value of the Date header field parameter in the incoming Invite.  The time value should be in the Numeric Date format defined in RFC 7519: number of seconds elapsed since 00:00:00 UTC, Thursday, 1 January 1970 not including leap seconds. |
| from | origAddress | Y | Represents the asserted identity of the originator of the personal communications signaling.  This is set to the value of the “P-Asserted-Identity”, if available, or “From” header field parameter in the incoming Invite. |
| displayName | String | N | The display name of the originator of the call, which the client may get from SIP signaling or other means. |
| profileid | String | N | Identifier of the profile in the profile table on the server to use for verifying this request.  This profile determines configuration used for verification, e.g. display name action, required IAT freshness. |
| requestid | String | N | An opaque identifier that is reflected in the response in order to make possible the transaction traceability in case of troubleshooting and fault analysis. |

## Datatype: verificationResponse

|  |  |  |  |
| --- | --- | --- | --- |
| Key Name | Key Value Type | Required? | Description |
| attest | String | N | SHAKEN extension to PASSporT.  Indicator identifying the service provider that is vouching for the call as well as clearly indicating what information the service provider is attesting to.  SHAKEN spec requires “attest” key value be set to uppercase characters “A”, “B”, or “C”. |
| origid | String | N | The unique origination identifier (“origid”) is defined as part of SHAKEN extension to PASSporT. This unique origination identifier should be a globally unique string corresponding to a UUID (RFC 4122). |
| displayname | String | N | Reflected from the request, and possibly modified based on the verification status. |
| errorid | String | N | Alphanumeric identifier indicating the nature of the error. |
| reasoncode | Integer | N | Reason Code to be used in case of failed verification by STI-VS to build SIP Reason header if required.  Currently possible values are defined as follows:  403,  428 (recommendation is to not use this Reason Code until a point where all calls on the VoIP network are mandated to be signed),  436,  437,  438 |
| reasontext | String | N | Reason Text to be used in case of failed verification by STI-VS to build SIP Reason header if required.  Currently possible values are defined as follows:  403 - “Stale Date”  428 - “Use Identity Header” (recommendation is to not use this Reason Text until a point where all calls on the VoIP network are mandated to be signed)  436 – “Bad Identity Info”  437 – “Unsupported Credential”  438 – “Invalid Identity Header” |
| reasondesc | String | N | Reason details description. Can be used for logging and troubleshooting. |
| verstat | String  {“TN-Validation-Passed”,  “TN-Validation-Failed”,  “No-TN-Validation”} | Y | Verification Status:  **TN-Validation-Passed** - The number passed the validation  **TN-Validation-Faile**d - The number failed the validation  **No-TN-Validation** - No number validation was performed |
| requestid | String | N | An opaque identifier that is reflected from the request in order to make possible the transaction traceability in case of troubleshooting and fault analysis. |

# Exceptions

RESTful services generate and send exceptions to clients in response to invocation errors. Exceptions send the relevant 4xx or 5xx HTTP status codes. HTTP status codes may be followed by details of the exception in the response body.

# API Interface

## Signing API

### Functional Behavior

Used to create the PASSporT signature with private key certificate.

The Authenticator sends a signing request including the following to the SHAKEN Signing Service:


1. The “orig” parameter is populated using the PAI field if present, otherwise using the From header field in the SIP Invite.
2. The “dest” parameter is populated using the To header field in the SIP Invite.
3. The “iat” parameter is populated using the “Date” header field in the SIP Invite. If there is no “Date” header field in the SIP Invite, a Date header field is added to the SIP INVITE.
4. If the required identity needs the SHAKEN extension:
   1. The "ppt" parameter is set to "shaken".
   2. The “origid” parameter is determined as described in ATIS-1000074 for the “origid” field in the PASSporT.
   3. The “attest” parameter is determined as described in ATIS-1000074 for the “attest” field in the PASSporT.
5. If the required identity needs the divert extension:
   1. The "ppt" parameter is set to "div".
   2. The "div" parameter is populated by determining where the call has been redirected from.
6. The "profileid" parameter is populated with the identifier of the profile the Authenticator wants to use to sign this PASSporT.
7. The "requestid" parameter is populated with an arbitrary identifier for this request that the Authenticator can use to correlate the response
8. The signingRequest is then sent to the SHAKEN Signing Service.

The SHAKEN Signing Service performs the following steps:

1. Validate the incoming signing request parameters in terms of parameter’s type and format.
2. Check the "profileid" in the request exists in the profile table. On failure, reject response (X3).
3. If there is no "profileid" in the request use the default one. If there is no default, reject the request (X4).
4. Validate the “iat” parameter value in terms of “freshness”: the request with “iat” value with time different by more than one minute from the current time will be rejected (E3).
5. Normalize to the canonical form the received telephony numbers if needed (remove visual separators and leading “+”) (X1 and X2).
6. Build SHAKEN PASSport protected JWT header (with “ppt” SHAKEN or divert extension).
7. Build SHAKEN PASSporT JWT payload by keeping lexicographic order and removing space and line breaking characters(X5).
8. Generate PASSporT signature with appropriate certificate private key.
9. Build Full Form of PASSporT.
10. Build SIP “Identity” header value by using identity digest from the previous step and add “info” parameter with angle bracketed URI used to acquire the public key of certificate used during PASSporT signing
11. If successfully signed, build and send “signingResponse” to the Authenticator, otherwise send error.

Upon receipt of the signingResponse, the Authenticator uses the “identity” parameter in the response to populate the SIP Identity header field and forwards the request. If no identity parameter is received in a response, the Authenticator forwards the request without adding a SIP Identity header field.

### Call Flow



### Request (POST)

The used resource is: http://{serverRoot}/stir/v1/signing.

|  |  |
| --- | --- |
| Name | Description |
| serverRoot | Server base URL: hostname+port+base path  Hostname contains the Global FQDN of Signing Service |

#### Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Signing Request | signingRequest | Yes | Contains the JSON structure of the signing request (PASSporT payload claims). |

#### Request Sample

POST /stir/v1/signing HTTP/1.1

Host: stir.example.com

Accept: application/json

X-InstanceID : de305d54-75b4-431b-adb2-eb6b9e546014

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"signingRequest”: {

"attest": “A”,

"orig”: {

“tn”: “12155551212”

},

“dest”: {

“tn”: [

“12355551212”

]

},

"iat”: 1443208345,

“origid”: “de305d54-75b4-431b-adb2-eb6b9e546014”

}

}

### Response

#### Response Body

Response body is returned as JSON object (Content-Type: application/json).

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Signing Response | signingResponse | Yes | Contains the JSON structure of the signing response (SIP Identity header field value). |

#### Response Sample (Success)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"signingResponse": {

"identity": “eyJhbGciOiJFUzI1NiIsInR5cCI6InBhc3Nwb3J0IiwicHB0Ijoic2hha2VuIiwieDV1IjoiaHR0cDov L2NlcnQtYXV0aC5wb2Muc3lzLmNvbWNhc3QubmV0L2V4YW1wbGUuY2VydCJ9eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6IisxMjE1NTU1MTIxMyJ9LCJpYXQiOiIxNDcxMzc1NDE4Iiwib3JpZyI6eyJ0biI64oCdKzEyMTU1NTUxMjEyIn0sIm9yaWdpZCI6IjEyM2U0NTY3LWU4OWItMTJkMy1hNDU2LTQyNjY1NTQ0MDAwMCJ9.\_28kAwRWnheXyA6nY4MvmK5JKHZH9hSYkWI4g75mnq9Tj2lW4WPm0PlvudoGaj7wM5XujZUTb\_3MA4modoDtCA;info=<<https://cert.example2.net/example.cert>>”

}

}

#### Response Sample (Failure)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"signingResponse": {

"errorid": "E3",

"reasoncode": 403,

"reasondesc": "Received \"iat\" value is not \"fresh\"",

"reasontext": "Stale Date"

}

}

### Request Bundle (POST)

The used resource is: http://{serverRoot}/stir/v1/signingBundle.

|  |  |
| --- | --- |
| Name | Description |
| serverRoot | Server base URL: hostname+port+base path  Hostname contains the Global FQDN of Signing Service |

#### Request Body

List of:

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Signing Request | signingRequest | Yes | Contains the JSON structure of the signing request (PASSporT payload claims). |

#### Request Sample

POST /stir/v1/signingBundle HTTP/1.1

Host: stir.example.com

Accept: application/json

X-InstanceID : de305d54-75b4-431b-adb2-eb6b9e546014

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

[

{

"signingRequest": {

"attest": "A",

"dest": {

"tn": [

"(+1)235-555-1212"

]

},

"iat": 1483228800,

"orig": {

"tn": "(+1)235-555-1212"

},

"origid": "8a8ec618-c6b9-30ae-b427-af4104b1c02c",

"ppt": "shaken",

"profileid": "1234",

"requestid": "1"

}

},

{

"signingRequest": {

"attest": "A",

"dest": {

"tn": [

"(+1)235-555-1212"

]

},

"iat": 1483228800,

"orig": {

"tn": "(+1)235-555-1212"

},

"origid": "8a8ec618-c6b9-30ae-b427-af4104b1c02c",

"ppt": "shaken",

"profileid": "2345",

"requestid": "2"

}

}

]

### Response

#### Response Body

Response body is returned as JSON array (Content-Type: application/json) of objects defined by the following:

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Signing Response | signingResponse | Yes | Contains the JSON structure of the signing response (SIP Identity header field value). |

#### Response Sample (Success)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

[

{

"signingResponse": {

"identity": "eyJhbGciOiJFUzI1NiIsInBwdCI6InNoYWtlbiIsInR5cCI6InBhc3Nwb3J0IiwieDV1IjoiaHR0cDovLzUyLjIzLjI1MC45Mzo4MDgwL2NlcnRzL3NoYWtlbi5jcnQifQ.eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6WyIxMjM1NTU1MTIxMiJdfSwiaWF0IjoxNDgzMjI4ODAwLCJvcmlnIjp7InRuIjoiMTIzNTU1NTEyMTIifSwib3JpZ2lkIjoiOGE4ZWM2MTgtYzZiOS0zMGFlLWI0MjctYWY0MTA0YjFjMDJjIn0.SdOwnT70ZZDAjgSmQVP-\_0keB\_pu4FjkBg5DZDyFf\_V5k0EUAY0KCHr2g2a6wOSs-JhsehdYUnrYCfkYItzxLg;info=<http://example1.com/certs/shaken.crt>;alg=ES256;ppt=shaken",

"requestid": "1"

}

},

{

"signingResponse": {

"identity": "eyJhbGciOiJFUzI1NiIsInBwdCI6InNoYWtlbiIsInR5cCI6InBhc3Nwb3J0IiwieDV1IjoiaHR0cDovLzUyLjIzLjI1MC45Mzo4MDgwL2NlcnRzL3NoYWtlbi5jcnQifQ.eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6WyIxMjM1NTU1MTIxMiJdfSwiaWF0IjoxNDgzMjI4ODAwLCJvcmlnIjp7InRuIjoiMTIzNTU1NTEyMTIifSwib3JpZ2lkIjoiOGE4ZWM2MTgtYzZiOS0zMGFlLWI0MjctYWY0MTA0YjFjMDJjIn0.SdOwnT70ZZDAjgSmQVP-\_0keB\_pu4FjkBg5DZDyFf\_V5k0EUAY0KCHr2g2a6wOSs-JhsehdYUnrYCfkYItzxLg;info=<http://example2.com/certs/shaken.crt>;alg=ES256;ppt=shaken",

"requestid": "2"

}

}

]

#### Response Sample (Failure)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

[

{

"signingResponse": {

"errorid": "E3",

"reasoncode": 403,

"reasondesc": "Received \"iat\" value is not \"fresh\"",

"reasontext": "Stale Date",

"requestid": "1",

}

},

{

"signingResponse": {

"errorid": "E3",

"reasoncode": 403,

"reasondesc": "Received \"iat\" value is not \"fresh\"",

"reasontext": "Stale Date",

"requestid": "2",

}

}

]

### Signing failure cases

| Error Case Number | Error Case  (“reasondesc”) | HTTP Status Code | ”reasoncode” | ”reasontext” |
| --- | --- | --- | --- | --- |
| E3 | Received ’iat‘ value is not fresh | 200 | 403 | Stale Date |
| X1 | Unexpected characters found in "tn" value in ["orig" / "dest" / "div"] parameter | 200 | 400 | Bad Request |
| X2 | Found both "tn" and "uri" values in ["orig" / "div"] parameter | 200 | 400 | Bad Request |
| X3 | Unrecognized "profileid" in request | 200 | 400 | Bad Request |
| X4 | No "profileid" in request and no default profile entry configured | 200 | 400 | Bad Request |
| X5 | Incorrect parameters supplied for given "ppt" value | 200 | 400 | Bad Request |

## Verification API

### Functional Behavior

The Verification API is used to verify the signature provided in the Identity header field and to determine that the signing service credentials demonstrate authority over the call originating identity.


Upon receipt of a SIP INVITE containing some SIP Identity header fields, the Verifier builds a verificationRequest as follows:

1. The “from” parameter is populated using the PAI field if present, otherwise using the From header field in the SIP Invite.
2. The “to” parameter is populated with the To header field from the SIP Invite.
3. The “time” parameter value is populated with the RFC7519 encoded Date header field from the SIP Invite.
4. The “identities” parameter value is populated using the Identity header fields in the SIP Invite.
5. The "displayname" parameter is populated using the From header field, or other implementation-defined source.
6. The "profileid" parameter is populated with the identifier of the profile the Verifier wants to use to verify this INVITE.
7. The "requestid" parameter is populated with an arbitrary identifier for this request that the Verifier can use to correlate the response.
8. The Verifier then sends the HTTP Post to request verification.

Upon receipt of the verification request, the SHAKEN Verification Service performs the following steps. Each step is associated with the appropriate error case(s) specified in the section “Mapping of verification failure cases to the returned SIP header parameters”. The error case numbers **En** per each step is specified in parentheses.

1. Validate the incoming verification request parameters in terms of parameter’s type and format (E1 and E2).
2. Check the "profileid" in the request exists in the profile table. On failure, reject response (X3).
3. If there is no "profileid" in the request use the default one. If there is no default, reject the request (X4).
4. Canonicalize the addresses in the "from" and "to" fields in the request. On failure, reject response (X2).
5. Validate the “time” parameter value in terms of “freshness”: a request with a “time” value which is different by more than one minute from the current time will be rejected (E3)
6. Parse each “identity” parameter value:
   1. full form of PASSporT is required by SHAKEN: “identity-digest” parameter of Identity header has to be parsed to validate the full form format [three data portions delimited with dot (“.”)]. If the expected format is not matched 🡪 reject identity on the Invalid PASSporT form (E4).
   2. If “ppt” parameter is specified and its value is not “shaken” 🡪 reject identity (E5).
   3. If “info” parameter is not specified 🡪 reject identity (E6).
   4. If the URI specified in “info” parameter is not syntactically valid 🡪 reject identity (E7).
7. Decode each “identity-digest” parameter value to extract from the first portion (PASSporT header) “ppt”, “typ”, “alg” and “x5u” claims:
   1. If one of the mentioned claims is missing -> reject identity (E9).
   2. If extracted “typ” value is not equal to “passport” 🡪 reject identity (E11).
   3. If extracted “alg” value is not equal to “ES256” 🡪 reject identity (E12) .
   4. If extracted “x5u” value is not equal to the URI specified in the “info” parameter of Identity header 🡪 reject identity (E10).
   5. If extracted “ppt” is not equal to “shaken” 🡪 reject identity (E13).
8. Decode each “identity-digest” parameter value to extract from the second portion (PASSporT payload) “dest”, “orig”, “attest”, “origid”, "div" and “iat” claims:
   1. On missing mandatory claims reject identity (E14).
   2. If "attest" and "origid" are not present and "ppt" is "shaken", or "div" is not present and "ppt" is "div" reject the identity (X5).
   3. Validate the addresses in the "orig", "dest", and "iat" claims, if they contain unexpected characters reject the identity (X1), if "orig" or "div" contain "tn" and "uri" claims, reject the identity (X2)
9. Dereference each “info” parameter URI to a resource that contains the public key of the certificate used by signing service to sign a request. If there is a failure to dereference the URI due to timeout or a non-existent resource the identity is rejected (E8).
10. Validate each issuing CA. On the failure to authenticate the CA (for example not valid, no root CA) the identity will be rejected (E17).
11. Validate the signature of “identity” digest parameter. On failure, reject the identity (E18).
12. Construct a chain out of the remaining valid identities as described in [draft-ietf-stir-passport-divert-08] Section 4.2. On failure, reject the request with a representative error.

### Call Flow



### Request (POST)

The used resource is: http://{serverRoot}/stir/v1/verification.

|  |  |
| --- | --- |
| Name | Description |
| serverRoot | Server base URL: hostname+port+base path.  Hostname contains the Global FQDN of Verification Service. |

#### Request Body

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Verification Request | verificationRequest | Yes | Contains the JSON structure of the verification request (PASSporT payload claims + identity header). |

#### Request Sample

POST /stir/v1/verification HTTP/1.1

Host: stir.example.com

Accept: application/json

X-InstanceID : de305d54-75b4-431b-adb2-eb6b9e546014

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

“verificationRequest”: {

“from”: {

“tn”: “12155551212”

},

“to”: {

“tn”: [

“12355551212”

]

},

“time”: 1443208345,

“identity”: “eyJhbGciOiJFUzI1NiIsInR5cCI6InBhc3Nwb3J0IiwicHB0Ijoic2hha2VuIiwieDV1IjoiaHR0cDov L2NlcnQtYXV0aC5wb2Muc3lzLmNvbWNhc3QubmV0L2V4YW1wbGUuY2VydCJ9eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6IisxMjE1NTU1MTIxMyJ9LCJpYXQiOiIxNDcxMzc1NDE4Iiwib3JpZyI6eyJ0biI64oCdKzEyMTU1NTUxMjEyIn0sIm9yaWdpZCI6IjEyM2U0NTY3LWU4OWItMTJkMy1hNDU2LTQyNjY1NTQ0MDAwMCJ9.\_28kAwRWnheXyA6nY4MvmK5JKHZH9hSYkWI4g75mnq9Tj2lW4WPm0PlvudoGaj7wM5XujZUTb\_3MA4modoDtCA;info=<<https://cert.example2.net/example.cert>>”

}

}

### Response

#### Response Body

Response body is returned as JSON object (Content-Type: application/son).

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Verification Response | verificationResponse | Yes | Contains the JSON structure of the verification response. |

#### Response Sample (Success + Successful Validation)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"verificationResponse": {

“verstat”: “TN-Validation-Passed”

}

}

#### Response Sample (Success + Failed Validation)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

{

"verificationResponse": {

“reasoncode”: 436,

“reasontext”: “Bad Identity Info”,

“reasondesc”: “Invalid ‘info’ URI”,

“verstat”: “No-TN-Validation”

}

}

### Request Bundle (POST)

The used resource is: http://{serverRoot}/stir/v1/verificationBundle.

|  |  |
| --- | --- |
| Name | Description |
| serverRoot | Server base URL: hostname+port+base path.  Hostname contains the Global FQDN of Verification Service. |

#### Request Body

Request body is a JSON array (Content-Type: application/json), with elements of type:

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Verification Request | verificationRequest | Yes | Contains the JSON structure of the verification request (PASSporT payload claims + identity header). |

#### Request Sample

POST /stir/v1/verificationBundle HTTP/1.1

Host: stir.example.com

Accept: application/json

X-InstanceID : de305d54-75b4-431b-adb2-eb6b9e546014

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

[

{

"verificationRequest": {

"dest": {

"tn": [

"(+1)235-555-1212"

]

},

"displayname": "James Smith",

"iat": 1483228800,

"identity": "eyJhbGciOiJFUzI1NiIsInBwdCI6InNoYWtlbiIsInR5cCI6InBhc3Nwb3J0IiwieDV1IjoiaHR0cDovLzUyLjIzLjI1MC45Mzo4MDgwL2NlcnRzL3NoYWtlbi5jcnQifQ.eyJhdHRlc3QiOiJBIiwiZGVzdCI6eyJ0biI6WyIxMjM1NTU1MTIxMiJdfSwiaWF0IjoxNDgzMjI4ODAwLCJvcmlnIjp7InRuIjoiMTIzNTU1NTEyMTIifSwib3JpZ2lkIjoiOGE4ZWM2MTgtYzZiOS0zMGFlLWI0MjctYWY0MTA0YjFjMDJjIn0.SdOwnT70ZZDAjgSmQVP-\_0keB\_pu4FjkBg5DZDyFf\_V5k0EUAY0KCHr2g2a6wOSs-JhsehdYUnrYCfkYItzxLg;info=<http://52.23.250.93:8080/certs/shaken.crt>;alg=ES256;ppt=shaken",

"orig": {

"tn": "(+1)235-555-1212"

},

"profileid": "1234",

"requestid": "1"

}

},

{

"verificationRequest": {

"dest": {

"tn": [

"(+1)235-555-1212"

]

},

"displayname": "James Smith",

"iat": 1483228800,

"identities": [

"eyJhbGciOiJFUzI1NiIsInBwdCI6InNoYWtlbiIsInR5cCI6InBhc3Nwb3J0IiwieDV1IjoiaHR0cDovLzUyLjIzLjI1MC45Mzo4MDgwL2NlcnRzL3NoYWtlbi5jcnQifQ.eyJhdHRlc3QiOiJCIiwiZGVzdCI6eyJ0biI6WyIxMjM1NTU1MTIxMiJdfSwiaWF0IjoxNDgzMjI4ODAwLCJvcmlnIjp7InRuIjoiMTIzNTU1NTEyMTIifSwib3JpZ2lkIjoiYTRmMjQ1NzktNDVkNS00MTUyLWFkZTUtYjllMzJhNDU4MTQ3In0.HQw5LtkQ4dVg9FdKbufGU1V31Ft6hCun\_eQpXDvUg7EE8jRZYegvM8YWOziR2hn4-GTxyLAEM2vBAO2dlqijIA;info=<http://52.23.250.93:8080/certs/shaken.crt>;alg=ES256;ppt=shaken",

"eyJhbGciOiJFUzI1NiIsInBwdCI6ImRpdiIsInR5cCI6InBhc3Nwb3J0IiwieDV1IjoiaHR0cDovLzUyLjIzLjI1MC45Mzo4MDgwL2NlcnRzL3NoYWtlbi5jcnQifQ.eyJkZXN0Ijp7InRuIjpbIjEyMzU1NTUxMjEyIl19LCJpYXQiOjE0ODMyMjg4MDAsIm9yaWciOnsidG4iOiIxMjM1NTU1MTIxMiJ9LCJkaXYiOiIxMjM1NTU1MTIxMiJ9.SdOwnT70ZZDAjgSmQVP-\_0keB\_pu4FjkBg5DZDyFf\_V5k0EUAY0KCHr2g2a6wOSs-JhsehdYUnrYCfkYItzxLg;info=<http://52.23.250.93:8080/certs/shaken.crt>;alg=ES256;ppt=div"

]

"orig": {

"tn": "(+1)235-555-1212"

},

"profileid": "1234",

"requestid": "2"

}

}

]

### Response Bundled

#### Response Body

Response body is returned as JSON array (Content-Type: application/json), with elements of type:

|  |  |  |  |
| --- | --- | --- | --- |
| Parameter | Data Type | Required? | Brief description |
| Verification Response | verificationResponse | Yes | Contains the JSON structure of the verification response. |

#### Response Sample (Success + Successful Validation)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

[

{

"verificationResponse": {

"attest": "A",

"displayname": "(Verified) James Smith",

"origid": "8a8ec618-c6b9-30ae-b427-af4104b1c02c",

"ppt": "shaken",

"requestid": "1",

"verstat": "TN-Validation-Passed"

}

},

{

"verificationResponse": {

"attest": "B",

"displayname": "(Verified) James Smith",

"origid": " a4f24579-45d5-4152-ade5-b9e32a458147",

"ppt": "shaken",

"requestid": "2",

"verstat": "TN-Validation-Passed"

}

}

]

#### Response Sample (Success + Failed Validation)

HTTP/1.1 200 OK

X-RequestID: AA97B177-9383-4934-8543-0F91A7A02836

Content-Type: application/json

Content-Length: …

[

{

"verificationResponse": {

"displayname": "Possible spam",

"errorid": "E10",

"reasoncode": 436,

"reasondesc": "\"x5u\" from PASSporT header doesn’t match the "info" parameter from \"identity\"",

"reasontext": "Bad Identity Info",

"requestid": "1",

"verstat": "No-TN-Validation"

}

},

{

"verificationResponse": {

"attest": "B",

"displayname": "(Verified) James Smith",

"origid": " a4f24579-45d5-4152-ade5-b9e32a458147",

"ppt": "shaken",

"requestid": "2",

"verstat": "TN-Validation-Passed"

}

}

]

### Verification failure cases

| Error Case Number | Error Case  (“reasondesc”) | HTTP Status Code | ”reasoncode” | ”reasontext” | “verstat” |
| --- | --- | --- | --- | --- | --- |
| E1 | Missing mandatory parameters in the verification request  (“from”, “to”,”time”, “identity”) | 400 with service exception | - | - | No-TN-Validation |
| E2 | Received invalid parameters  (invalid “from”/”to” tn format, “time” value) | 400 with service exception | - | - | No-TN-Validation |
| E3 | Received ’iat‘ value is not fresh | 200 | 403 | Stale Date | No-TN-Validation |
| E4 | Identity header in compact form instead of required by SHAKEN spec full form. | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E5 | Identity header is received with ’ppt‘ parameter value that is not ‘shaken’ | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E6 | Missing ‘info’ parameter in the ‘identity’ | 200 | 436 | Bad identity Info | No-TN-Validation |
| E7 | Invalid ‘info’ URI | 200 | 436 | Bad identity Info | No-TN-Validation |
| E8 | Failed to dereference ‘info’ URI | 200 | 436 | Bad identity Info | No-TN-Validation |
| E9 | Missing ‘%1’ claim in the PASSporT header  %1 - “ppt”, ”typ”, ”alg”, ”x5u” | 200 | 436 | Bad identity Info | No-TN-Validation |
| E10 | ‘x5u’ from PASSporT header doesn’t match the ‘info’ parameter of identity header value | 200 | 436 | Bad identity Info | No-TN-Validation |
| E11 | ‘typ’ from PASSporT header is not ‘passport’ | 200 | 437 | Unsupported credential | No-TN-Validation |
| E12 | ‘alg‘ from PASSporT header is not ‘ES256’ | 200 | 437 | Unsupported credential | No-TN-Validation |
| E13 | ‘ppt‘ from PASSporT header is not ‘shaken’ | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E14 | Missing ‘%1’ mandatory claim in PASSporT payload  %1 - “dest”, “orig”, “attest”, “origid”, ”iat” | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E15 | ‘iat’ from PASSporT payload is not fresh | 200 | 403 | Stale Date | No-TN-Validation |
| E16 | ‘%1’ claim from PASSporT payload doesn’t match the received in the verification request claim  %1 - “orig”, “dest” | 200 | 438 | Invalid Identity Header | No-TN-Validation |
| E17 | Failed to authenticate CA | 200 | 437 | Unsupported credential | TN-Validation-Failed |
| E18 | Signature validation failed | 200 | 438 | Invalid Identity Header | TN-Validation-Failed |
| X1 | Unexpected characters found in "tn" value in ["orig" / "dest" / "div"] parameter | 200 | 400 | Bad Request | No-TN-Validation |
| X2 | Found both "tn" and "uri" values in ["orig" / "div"] parameter | 200 | 400 | Bad Request | No-TN-Validation |
| X3 | Unrecognized "profileid" in request | 200 | 400 | Bad Request | No-TN-Validation |
| X4 | No "profileid" in request and no default profile entry configured | 200 | 400 | Bad Request | No-TN-Validation |
| X6 | Too many identities in request | 200 | 400 | Bad Request | No-TN-Validation |

1. This document is available from the Internet Engineering Task Force (IETF). < <http://www.ietf.org> > [↑](#footnote-ref-1)
2. This document can be found at < <https://datatracker.ietf.org/doc/draft-wendt-stir-passport-shaken/> >. [↑](#footnote-ref-2)
3. This document is available from the Internet Engineering Task Force (IETF). < <http://www.ietf.org> > [↑](#footnote-ref-3)
4. This document is available from the Alliance for Telecommunications Industry Solutions (ATIS) at < <https://www.atis.org/docstore/product.aspx?id=28297> >. [↑](#footnote-ref-4)
5. This document is available from the Alliance for Telecommunications Industry Solutions (ATIS) at < <https://www.atis.org/docstore/product.aspx?id=28345> > [↑](#footnote-ref-5)